**Aga Khan Rural Support Program (AKRSP)**

**REQUEST FOR QUOTATION (RFQ)**

**RFQ No:** 0091/25   
**RFQ Date:** March 17, 2025   
**Submission Date:** April 03, 2025  
**Delivery Point:** Phurkhot, Torkhow, Upper Chitral

**Subject: Request For Quotation**

Aga Khan Rural Support Program (AKRSP) invites qualified service providers to submit sealed quotations for the “**Supply and Transportation of Conductors and Other T&D Items for Phur Khot MHP”** of 100kW capacity at Phurkhot, Torkhow, Upper Chitral.The following Request for Quotation (RFQ) details the scope of requirements, terms & conditions, and evaluation criteria. Please carefully review and comply with the specifications outlined in this document.

**Scope of Requirements:** Vendors must thoroughly understand and comply with the requirements as outlined in the terms of reference. Any clarifications needed should be requested within the specified timeline.

**Terms & Conditions for Submission of Sealed Quotations:**

**Submission Requirements:** Quotations must be submitted on the company/organization’s official letterhead with a date, signature, and stamp.

**Compliance and Evaluation:** Quotations must meet all specifications, requirements, and offer the lowest price along with fulfilling other evaluation criteria. Non-compliant offers will be rejected.

**Price Calculation:** Any discrepancies between unit prices and total prices will be recalculated by AKRSP, with the unit price prevailing. Suppliers must accept the corrected total price to avoid rejection.

**Price Variation:** No price variations due to market factors will be accepted after quotation submission. AKRSP reserves the right to adjust the quantity without changing unit prices or terms at the time of awarding the contract.

**Non-Binding:** AKRSP is not obligated to accept any quotation or award a contract. Suppliers are responsible for all costs associated with quotation preparation and submission.

**Conflict of Interest:** AKRSP emphasizes transparency and integrity. Vendors must disclose any conflicts of interest, including direct or indirect involvement of the vendor or its affiliates in preparing RFQ details. This ensures a fair process. We maintain zero tolerance for fraud and unethical practices, committed to upholding honesty, accountability, and compliance with our vendors.

**Transportation Responsibility:** Suppliers are responsible for safely transporting all materials to the project site.

**Travel and Accommodation:** Suppliers must arrange their travel, accommodation, and meals during the supply and installation period.

**Design Compliance:** All supplied items must adhere to approved and reliable design standards.

**Inspection and Rejection:** Materials will undergo inspection either at Chitral or the project site. Deviations from specified specifications can lead to material rejection, with the supplier bearing replacement costs.

1. Evaluation of bids shall be carried out in two stages:

**Technical Evaluation:** In this stage the bidder shall be evaluated on the following criteria on “Pass” or “Fail” basis:

**Work Experience:** The Bidder shall present a minimum of one reference on assignments of similar size and nature:

An aggregate experience of works involving Electrical/Transmission & Distribution work supply/installations of the size. Satisfactory completion of at least one project of the same nature as a whole or multiple assignments in piecemeal aggregate, at least PKRs 20 million contract value each in the past 12 years, must be produced with bidding documents.

Or Joint Venture through a proper JV deed between firms with leading partner qualifying the work experience and supporting partner qualifying financial capability requirement may apply. Detailed project completion certificate/contract agreement specifying contract value to be attached as evidence.

**Financial Capability:**

The annual turnover for the last 03 years should be at least 20 million. This should be supported by original banks statements or true copy of audited financial statements.

The technically qualified bidder shall be financially evaluated, and lowest bidder shall be awarded the contract.

**Payment Terms:** Payments will be made in two instalments:

* 50% after material delivery to Chitral and inspection.
* 50% after material delivery to the project site.

**Taxes:** Quoted prices should be inclusive of all taxes.

**Mobilization Advance:** If requested, a mobilization advance requires a bank guarantee or call deposit equal to the advance amount.

**Rate Discrepancies:** Significant rate differences between quoted and market rates may lead to bid disqualification or procurement cancellation, and cartelization will result in backlisting. The same entity or individual can’t submit quotations under a different name.

**Validity Period:** Quoted rates should remain valid for Forty-Five (45) days.

**Cancellation Rights:** AKRSP reserves the right to cancel the complete procurement process or any particular item in the BOQ at any stage without specifying reasons.

**Delivery & Installation Timeline:** Services must be delivered in 45 days of agreement signing.

**Submission Deadline:** Sealed quotations must be submitted by hand or courier to Admin & Procurement Officer AKRSP Regional Office Shahi Qila Chitral by **COB April 03, 2025**

**Description of Works: “Supply and Transportation of Conductors and Other T&D Items for Phur Khot MHP”** at Phurkhot Torkhow, Upper Chitral**.**

**BOQ Table**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **S. N** | **Item Description** | **Specifications** | **Quantity** | **Unit** |
| 1 | AAC (ANT) Conductor | AAC Aluminum Conductor (LT) 50mm², Approx weight 145kg/km, DC resistance 0.54Ω/km. FAST, AGE, NEW AGE, Pakistan Cables Brands. | 55,000 | Meters |
| 2 | ACSR (Gopher) Conductor | ACSR Aluminum Conductor Steel Reinforced (HT) Gopher 25mm², Approx weight 106kg/km, DC resistance 1.09Ω/km. FAST, AGE, NEW AGE, Pakistan Cables Brands. | 36,000 | Meters |
| 3 | D fuse Set | D Fuse complete Set WAPDA Standard, EMCO or FICO or AH Associates original brand with Challan and Factory test report. | 10 | Set |
| 4 | Support Clamps | Hot-dipped Galvanized Support Clamps, WAPDA Standard, suitable for Gopher and Rabbit Conductor, 6mm thick steel, zinc coating ≥85 microns. | 60 | Nos |
| 5 | D Shackle Insulators | D-Shackle Insulator with Pin, Nut, Bolts, and Washer Complete Set. WAPDA Standard. Galvanized (hot-dipped) with min. 7-8mm thick steel. | 950 | Nos |
| 6 | Four Core Cable | Four Core Aluminum Cable 50mm² for step-down Transformer connections | 60 | Meters |
| 7 | Plate type Earthing System | Copper Earthing Plate 1x1ft, 8mm thick, Bolted arrangement, Includes 50ft Copper Wire (6 SWG) & Earthing Powder. WAPDA Standard | 1 | Set |
| 8 | GI Pipe | GI Pipe 1" dia, Medium Class (M), IIL Brand. Galvanized as per ASTM A53. | 20 | Rft |
| 9 | Rod type earthing | Copper Earth Rod, 8ft long, 20mm dia, with tapered design and clamp-on arrangement. Includes 100ft Copper Wire (6 SWG). | 8 | Set |
| 10 | Galvanized Steel Tripod for Chain Block | Heavy-duty galvanized Steel Tripod with Base Plate & Cross Bracing, hoisting mechanism, Load Capacity: 5 Tons, Height: 10ft. | 1 | No |
| 11 | Foldable Ladder | Aluminum Alloy 6063-T5 (Corrosion-resistant). Length: 20ft. Heavy duty. Weight: ~12kg. Step Width: 40-50mm. Anti-slip rubber feet, reinforced hinges, double-lock system. Standard: PSQCA / EN 131. | 1 | L/S |
| 12 | Fire Extinguisher | Powder Fire Extinguisher, 4KG, ABC Type, Certified by PSQCA, with wall mount or trolley option. | 1 | No |
| 13 | Safety Hat | Hard Safety Helmet with Adjustable Knob, CE Certified, ABS Material, Red and White Colors. | 5 | No |
| 14 | Safety Glasses | Safety Glasses with Adjustable Head Strap, ANSI Z87.1 Certified, Anti-fog, UV Protection. | 2 | No |
| 15 | Warning Signs | High Voltage and Moving Parts Warning Signs, 12x16 inch, SWG 20, Rust-proof GI/Steel sheet, Reflective paint, Urdu & English text. | 2 | No |
| 16 | Safety Ropes | High-strength Polypropylene Safety Rope, 12mm dia, Weather-resistant, Breaking strength ≥ 22kN, Chinese or WAPDA-approved brand. | 25 | Meter |
| 17 | Hot Stick | WAPDA Standard Fiberglass Hot Stick Rod, 12ft long, Non-conductive, Lightweight, Suitable for 11kV fuse link disconnection, Telescopic preferred. Standard: WAPDA Specification / IEEE 516 | 1 | No |
| 18 | Safety Vests | High-Visibility Safety Vest, Reflective Strips (Front & Back), Fluorescent Yellow or Orange, Adjustable, Made of durable polyester mesh, Chinese or WAPDA-approved brand. | 4 | No |
| 19 | Thickness Gauge | Digital Ultrasonic Thickness Gauge (Branded), Measuring range 1mm to 200mm+, Accuracy ±0.01mm, Calibration Certificate required. | 1 | No |
| 20 | Transportation Cost | Safe Transportation Cost of all equipment from Suppliers' premises to the Site, road type will include Jeepable transport to the site. Distance from Chitral Town 150km Phur Khot, Torkhow, Upper Chitral. | 1 | L/S |

Head of Admin & Procurement Vendor Receipt & Acknowledgement

AKRSP Head Office Gilgit

Sign and Stamp: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_