**Aga Khan Rural Support Program (AKRSP)**

**REQUEST FOR QUOTATION (RFQ)**

**RFQ No:** 0243/25   
**RFQ Date:** June 20, 2025  
**Submission Date:** June 30, 2025  
**Delivery Point:** Boliogh, Lower Chitral

**Subject: Request For Quotation**

The Aga Khan Rural Support Programme (AKRSP) invites sealed quotations from eligible and qualified service providers for the Supply and Transportation of Transmission & Distribution (T&D) Equipment for the 500kW Boliogh Micro Hydel Project (MHP) located in Boliogh, Lower Chitral. This Request for Quotation (RFQ) outlines the scope of work, terms and conditions, and evaluation criteria. Interested bidders are advised to carefully review and adhere to the specifications provided in this document.

**Scope of Requirements:** Vendors must thoroughly understand and comply with the requirements as outlined in the terms of reference. Any clarifications needed should be requested within the specified timeline.

**Terms & Conditions for Submission of Sealed Quotations:**

**Submission Requirements:** Quotations must be submitted on the company/organization’s official letterhead with a date, signature, and stamp.

**Compliance and Evaluation:** Quotations must meet all specifications, requirements, and offer the lowest price along with fulfilling other evaluation criteria. Non-compliant offers will be rejected.

**Price Calculation:** Any discrepancies between unit prices and total prices will be recalculated by AKRSP, with the unit price prevailing. Suppliers must accept the corrected total price to avoid rejection.

**Price Variation:** No price variations due to market factors will be accepted after quotation submission. AKRSP reserves the right to adjust the quantity without changing unit prices or terms at the time of awarding the contract.

**Non-Binding:** AKRSP is not obligated to accept any quotation or award a contract. Suppliers are responsible for all costs associated with quotation preparation and submission.

**Conflict of Interest:** AKRSP emphasizes transparency and integrity. Vendors must disclose any conflicts of interest, including direct or indirect involvement of the vendor or its affiliates in preparing RFQ details. This ensures a fair process. We maintain zero tolerance for fraud and unethical practices, committed to upholding honesty, accountability, and compliance with our vendors.

**Transportation Responsibility:** Suppliers are responsible for safely transporting all materials to the project site.

**Travel and Accommodation:** Suppliers must arrange their travel, accommodation, and meals during the supply and installation period.

**Design Compliance:** All supplied items must adhere to approved and reliable design standards.

**Inspection and Rejection:** Materials will undergo inspection either at Chitral or the project site. Deviations from specified specifications can lead to material rejection, with the supplier bearing replacement costs.

1. Evaluation of bids shall be carried out in two stages:

**Technical Evaluation:** In this stage the bidder shall be evaluated on the following criteria on “Pass” or “Fail” basis:

**Work Experience:**  
Bidders must provide at least one reference for assignments of similar size and nature. This includes cumulative experience in Electrical/Transmission & Distribution supply and installation works. The bidder must have successfully completed at least one project of similar scope with a minimum contract value of PKR 7.5 million, or multiple smaller projects that collectively meet or exceed this value, within the last five (05) years. Relevant documentation—such as detailed project completion certificates or contract agreements clearly indicating the contract value—must be submitted as part of the bidding documents.

**Financial Capability:**  
The bidder must have an average annual turnover of at least PKR 10 million over the last two (02) years. This must be supported by original bank statements or certified copies of audited financial statements.

**Evaluation Criteria:**  
Only technically qualified bidders will proceed to financial evaluation. The contract will be awarded to the lowest evaluated bidder.

**Payment Terms:** Payments will be made in two instalments:

* 50% after material delivery to Chitral and inspection.
* 50% after material delivery to the project site.

**Taxes:** Quoted prices should be inclusive of all taxes.

**Mobilization Advance:** If requested, a mobilization advance requires a bank guarantee or call deposit equal to the advance amount.

**Rate Discrepancies:** Significant rate differences between quoted and market rates may lead to bid disqualification or procurement cancellation, and cartelization will result in backlisting. The same entity or individual can’t submit quotations under a different name.

**Validity Period:** Quoted rates should remain valid for Thirty (30) days.

**Cancellation Rights:** AKRSP reserves the right to cancel the complete procurement process or any particular item in the BOQ at any stage without specifying reasons.

**Delivery & Installation Timeline:** Services must be delivered in 20 days of agreement signing.

**Submission Deadline:** Sealed quotations must be submitted by hand or courier to Regional Office AKRSP near Shahi Qilla Chitral by **COB June 30, 2025**.

**Description of Works: “Supply and Transportation of T&D Equipment for Boliogh 500KW MHP”** at Boliogh, Lower Chitral**.**

**BOQ Table**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **S. No** | **Item Description** | **Specifications** | **Quantity** | **Unit** | **Unit Rate** | **Total Amount** |
| 1 | ACSR Conductor Gopher | (ACSR) Aluminium Conductor Steel Reinforced (HT) Gopher 25mm2, Approx weight 106kg, DC resistance 1.09 ohm/km, Current Rating 126Amps FAST, AGE, NEW AGE or Pakistan Cable Brand | 12000 | Meters |  |  |
| 2 | 11 KV Pin insulator | • 11 KV Pin insulators with pin nut bolts complete as per WAPDA Standard • EMCO or FECO Made | 15 | No |  |  |
| 3 | Step down transformers 50kVA | 11/0.4 kV step down, connection HV: Delta, Connection LV: Star, with electrolytic copper winding, ONAN Cooled, one-year replacement warranty | 2 | No |  |  |
| 4 | De Fuse complete Set | • With Brass contactor • made of quality brand WAPDA Approved with delivery challan and factory test report must be produced | 2 | Sets |  |  |
| 5 | wooden cross arms | • 5'deodar wood with 4”x4” Cross section with no cracks or deformation. | 5 | No |  |  |
| 6 | Iron pole (LT) | MS Electric Poles 25ft Long @ 10ft 6inch dia, 10ft 5-inch dia and 5ft 4inch dia 4mm thick with hole for HT and LT insulators. Two holes at the base of the pole with 2 Nos of 18-inch-long, 0.5 inch dia steel rod provided for additional support, and Blue Color paint. Approx weight 102kg | 45 | No |  |  |
| 7 | Brace for wooden cross arms | Hot dipped GI, Cross arm brace 25inch length, 2inch width and 9mm thickness. Average weight 2.27kg. Two number of 6 inch long bolts with nut and washers, One 7 inch long bolt with nut and washer and one 12 inch long bolt 0.5 inch dia along with nut and washers. | 10 | No |  |  |
| 8 | D-shackle, spool insulator | D-shackle Insulator with D 6mm Pin 4 inch, Nut Bolts 7inch and Washer Complete set WAPDA Standard | 140 | No |  |  |
| 9 | 4-Core cable | (50mm square) Al core, insulated cable for Transformer connection | 12 | Meters |  |  |
| 10 | Transportation Cost of T&D equipment | Transportation of T & D equipment to site at Bohtuli village end near Parsan Valley jeepable transport | 1 | L/S |  |  |

Admin & Procurement Officer Vendor Receipt & Acknowledgement

AKRSP Chitral

Sign and Stamp: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_