**Aga Khan Rural Support Program (AKRSP)**

**REQUEST FOR QUOTATION (RFQ)**

**RFQ No:** AKRSP/ 192 /2025 **Delivery Point: Yukum, Lower Yarkhoon, Upper Chitral**

**RFQ Date: May 15, 2025 Submission Date: May 28, 2025**

**Subject: Request For Quotation**

The Aga Khan Rural Support Programme (AKRSP) is a non-profit development organization working across the mountainous regions of Gilgit-Baltistan and Chitral to improve the quality of life for rural communities. AKRSP implements participatory development initiatives in multiple sectors, including infrastructure development, agriculture, renewable energy, and livelihoods. In line with this mission, AKRSP invites sealed quotations from reputable, experienced, and qualified suppliers for the supply & transportation of HDPE Pipes, steel wire rope & accessories and installation of HDPE Pipes at Yukum, Lower Yarkhoon, Upper Chitral.

This Request for Quotation (RFQ) outlines all requirements, submission guidelines, terms and conditions, and evaluation criteria necessary for a fair and competitive selection process. Vendors are advised to read this document thoroughly and ensure complete compliance before submitting their bids.

**Terms & Conditions for Submission of Sealed Quotations:**

* **Submission Requirements:** Quotations must be submitted on the company/organization’s official letterhead with a date, signature, and stamp.
* **Compliance and Evaluation:** Quotations must meet all specifications, requirements, and offer the lowest price along with fulfilling other evaluation criteria. Non-compliant offers will be rejected.
* **Price Calculation:** Any discrepancies between unit prices and total prices will be recalculated by AKRSP, with the unit price prevailing. Suppliers must accept the corrected total price to avoid rejection.
* **Price Variation:** No price variations due to market factors will be accepted after quotation submission. AKRSP reserves the right to adjust the quantity without changing unit prices or terms at the time of awarding the contract.
* **Non-Binding:** AKRSP is not obligated to accept any quotation or award a contract. Suppliers are responsible for all costs associated with quotation preparation and submission.
* **Conflict of Interest:** AKRSP emphasizes transparency and integrity. Vendors must disclose any conflicts of interest, including direct or indirect involvement of the vendor or its affiliates in preparing RFQ details. This ensures a fair process. We maintain zero tolerance for fraud and unethical practices, committed to upholding honesty, accountability, and compliance with our vendors.
* **Transportation Responsibility:** Suppliers are responsible for safely transporting all materials to the project site.
* **Travel and Accommodation:** Suppliers must arrange their travel, accommodation, and meals during the supply and Transportation period.
* **Design Compliance:** All supplied items must adhere to approved and reliable design standards.
* **Inspection and Rejection:** Materials will undergo inspection either at Chitral or the project site. Deviations from specified specifications can lead to material rejection, with the supplier bearing replacement costs.
* **Evaluation Criteria:** The evaluation process will include a thorough financial assessment of the bids. The contract will be awarded to the bidder with the lowest bid price, provided they meet all the requirements specified in the RFQ document.
* **Payment Terms:** Payments will be made in three instalments:
	+ 50% after material delivery to Chitral and inspection.
	+ 40% after material delivery to the project site.
	+ 10% after Installation of Pipes & Accessories
	+ All payments will be made through cross cheque within 15 working days upon submission of invoice and verification of deliverables.
* **Taxes and Duties:** Quoted prices must be inclusive of all applicable taxes, duties, and government levies.
* **Rate Discrepancies:** Significant rate differences between quoted and market rate may lead to procurement cancellation.
* **Validity Period:** Quoted rates should remain valid for at least one month starting from last date of bid submission.
* **Cancellation Rights:** AKRSP reserves the right to cancel the procurement process at any stage without specifying reasons.
* **Delivery & Installation Timeline:**
	+ Supply and transportation must be delivered within 30 days of the agreement signing.
	+ Installation of pipes should be completed within 30 days upon completion of pipe crossing structure above Yarkhoon river at Yukum.
* **Cartelization**: Any evidence of collusion or multiple quotations from the same entity under different names will result in blacklisting and disqualification.
* **Rejection Rights**: AKRSP reserves the right to reject any or all bids without assigning any reason.
* **Fraud and Corruption**: AKRSP maintains zero tolerance towards fraud, bribery, and unethical practices. Any vendor found violating these principles will be permanently disqualified.
* **Amendments**: AKRSP may issue an amendment or addendum to this RFQ if needed. All potential vendors will be informed.
* **Force Majeure**: AKRSP shall not be liable for any delay or failure to perform resulting from events beyond reasonable control, including but not limited to natural disasters, war, civil unrest, etc.
* **Subcontracting**: No subcontracting is allowed without prior written consent from AKRSP.
* **Dispute Resolution**: Any disputes arising shall be resolved through mutual consultation. Failing which, arbitration laws of Pakistan will apply.
* **Ownership**: All items supplied will become the property of AKRSP after final acceptance.

**Submission Deadline:** Sealed quotations must be submitted by hand or courier to AKRSP Regional Program Office near Shahi Qilla Chitral by COB May 28, 2025

Zakir Hussain Vendor Receipt & Acknowledgement

AKRSP Chitral

 Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

 Designation: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Sign & Stamp

**Description of Works:** **Supply & transportation of HDPE Pipes, steel wire rope & accessories and installation of HDPE Pipes at Yukum, Lower Yarkhoon, Upper Chitral.**

**BOQ Table**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Sr. No.** | **Item Description** | **Units** | **Quantity** | **Unit Price (PKR)** | **Total Price (PKR)** |
| 1 |  HDPE Pipe, (PN-10) PE-100, 160mm outer Diameter, Single Pipe Length= 20 rftApproved Manufacturers: Dadex, IIL, Royal, Sun International, Jamal | RFT | 3,760 |  |   |
| 2 | Stub end, 6 inch Diameter | No | 20 |  |  |
| 3 | Flange, 12mm thick, 6 Inch Diameter | No | 20 |  |  |
| 4 | Rubber Packen, 8mm thick | No | 13 |  |  |
| 5 | Nut Bolts, 1/2 inch Dia, 4 inch length for stub ends | No | 78 |  |  |
| 6 | Equal Tee , HDPE PN-10 , PE-100 160mm Dia | No | 1 |  |  |
| 7 | 6" Flushing ValveBy Mughul or Anwar | No | 1 |  |  |
| 8 | 4" GI PipeMedium Class  | RFT | 5 |  |  |
| 9 | 4" Gate Valve (For GI Pipe)By Mughul or Anwar | No | 1 |  |  |
| 10 | 6" Gate Valve (For MS Pipe)By Mughul or Anwar | No | 1 |  |  |
| 11 | Air Valve1” Italian | No | 1 |  |  |
| 12 | Saddle Clamp | No | 1 |  |  |
| 13 | 6" MS Pipe w/ Equal Dia Flange Welded to One EndWall Thickness 4mm4.7 Kg/Ft | RFT | 5 |  |  |
| 14 | IWRC 6\*19 New Steel wire rope, 1 inch Dia, Steel Core (0.839kg/ft)Extra Improved Plowed Steel (EIPS) | RFT | 380 |  |  |
| 15 | IWRC 6\*19 New Steel wire rope, 1/2 inch Dia, Steel Core (0.24kg/ft)Extra Improved Plowed Steel (EIPS) | RFT | 2600 |  |  |
| 16 | Steel Girder (6"x3"), L=4 ft, weight =5.25 kg/ft (02 No)Web Thickness – 6 mmFlange Thickness – 8 mm | KG | 42 |  |  |
| 17 | Steel Girder (6"x3"), L=2 ft, weight =5.25 kg/ft (04 No)Web Thickness – 6 mmFlange Thickness – 8 mm | KG | 42 |  |  |
| 18 | Anchorage Rods, Diameter =1-1/4 inch, L=4 ft weight=1.9kg/ft (04 No) | KG | 30 |  |  |
| 19 | Anchorage Rods, Diameter =1-1/4 inch, L=2 ft weight=1.9kg/ft (04 No) | KG | 15 |  |  |
| 20 | Bulldog Grips, 12 mm Dia heavy duty. | No | 256 |  |  |
| 21 | Bulldog Grips, 22 mm Dia heavy duty. | No | 240 |  |  |
| 22 | Bulldog Grips, 28mm Dia heavy duty. | No | 8 |  |  |
| 23 | Installation charges of Pipes and fittings only. | LMS | 1 |  |  |
| 24 | Transportation Cost includes Loading/Unloading | LMS | 1 |  |  |
| **Total cost** |   |
| **GST if applicable** |   |
| **Grand Total including** |   |
| **Note:**Quoted cost should include all associated costs including supply & transportation of above-mentioned items Plus Installation of HDPE Pipes & fittings only. |   |